Updater Program Firmware Update Limitations:
1. Only supports devices with MCU and FPGA versions 0.55.0 or higher, and Bus version 0.55.3 or higher .
2. If the Updater program terminal displays a message related to 200-ohm resistance, this device is not supported for using the Updater. Please contact technical support.
3. NX series devices are not supported for using the Updater. Please contact technical support.
4. PX series devices currently only support the following firmware version combinations for upgrades:
MCU      FPGA
0.55.54   0.55.22
0.55.53   0.55.22
0.55.50   0.55.18
0.55.49   0.55.18
0.55.48   0.55.18
0.55.48   0.55.17
0.55.46   0.55.17
0.55.45   0.55.17
0.55.45   0.55.15
0.55.40   0.55.15
0.55.39   0.55.15
0.55.38   0.55.15

Update Steps
PX Series Device Update on Linux System:
1.Extract the files and copy them to the desktop of the PX series instrument.
2. Click the "updater" icon in the "Updater_0_55_XX_vX" folder. The terminal will display the current firmware version of the device and the firmware version in the update program. After confirming everything is correct, press Enter to start the update.
3. During the update process, please patiently wait according to the progress bar until the update is complete.
4. After closing the program, open the software, click "System"→ "About", and check whether the MCU and FPGA of the instrument are updated.
Note: After upgrading the FX3 on PX devices, please ensure the device is powered off for at least 8 seconds before restarting. You can check if the Bus is updated by clicking "System" → "About".


